Main applications:
Water supply pipes and drinking water pipes in buildings;
Cold water supply pipes in buildings;
Gas delivery pipes of LPG, LNG etc;

Product performance:
Temperature and Pressure Resistance: max. up to 60℃,1-1.25Mpa.
High Mechanical Strength: not easy to be damaged or cracked.
Corrosion Resistance: resistant to acid, alkaline and salt solutions.
Cleanness and Health: no harmful substances, mould-proof, non-rusting and non-scaling.
Light Weight: arbitrary length with convenient installation.
Flexibility and Non-Rebound: can be bent without being heated, reduced the use of fittings.
Heat Preservation: 1/100 heat conductivity of metal pipe, excellent heat preservation and outstanding energy conservation.
Anti-Vibration and Impact Resistance: the composite material can effectively reduce and absorb the pipe vibration so as to lower the noise.